DMX Processor 8000
A. General:
1. The DMX processor shall be a DMX Processor 8000. The DMX Processor shall be available from High End Systems, Inc., 2105 Gracy Farms Lane, Austin, TX 78758, USA.
2. The lighting control system shall be designed specifically for the control of stage, studio, touring, entertainment and architainment lighting systems.
3. A company having over 20 years of experience in the control of entertainment lighting shall manufacture the lighting control system.
4. The equipment shall be ETL listed.
5. Systems that do not provide the features listed below shall not be acceptable.
B. Hardware:
1. The DMX Processor shall be a 1U 483mm/19" rack unit, 280mm/11" deep, with a machined aluminum face panel with wear-resistant anoprinted legends.
2. The DMX Processor shall contain software controlled fans.
3. A universal 100-250V 50/60Hz power factor corrected power supply shall be incorporated.
4. Two (2) Gigabit Ethernet connections using rugged Neutrik etherCON connectors, allowing for HogNet and FixtureNet capability.
5. The DMX Processor shall have two (2) USB A connections on the rear panel.
6. The DMX Processor shall have a locking IEC power connection on the rear panel.
7. There shall be eight (8) isolated DMX512 ports on the front of the unit.
C. Operation
1. The Hog 4 control system shall be expandable through the use of multiple DMX processor units.
2. In normal operation it shall be connected to a Wholehog III series or Hog 4 series console or other HOG compatible server by an Ethernet network.
3. The DMX XLR output shall be expandable via USB Widgets, USB Super Widgets or a USB Super Duper Widget.
4. The firmware shall be upgradeable over the network. No changing of internal components shall be required.
5. There shall be a user interface comprising a color LED backlit graphic screen and three function buttons. There shall be LEDs on the front panel giving essential status information.
6. There shall be the option to connect up to eight (8) USB MIDI/LTC Timecode Widgets to each DMX 8000 processor.
D. Provide the following
Qty 	Part number 	Description
- 	61020004 	Hog 4 console in road case 
-	61020005	Full Boar 4 console in road case
-	61020006	Road Hog 4 console
-	61020011	HedgeHog 4 console
-	61020014	HedgeHog 4X console
- 	62040004 	DMX Processor 8000 (8192 channels, rack mount)
- 	74040007 	USB DMX Widget 
- 	74040008 	USB Super Widget 
- 	62040005 	USB DMX Super Duper Widget
- 	74040009 	USB MIDI/LTC Widget 
-	61040060 	Playback Wing 4
- 	61040062 	Master Wing 4
-	61040065	MiniWing 4
-	61040064	Hoglet 4 programming wing
- 	90903067 	Hog USB show storage flash drive (black)
- 	90903068 	Hog USB system restore flash drive (red)
- 	61040109 	Super Widget expansion kit
-	74040010	MIDI/LTC expansion kit
- 	61070012 	Playback/Master Wing 4 road case
-	61070011	Road Hog 4 road case
-	99330191	HedgeHog 4 soft carry bag
-	61070015	HedgeHog 4 Gator hard case
-	61070014	HedgeHog 4 custom road case
-	61070016	Hoglet 4 road case
-	61070017	MiniWing 4 road case
- 	61100004 	Hog white/blue desk light (extra)