Part 1.	Automated Lighting
1.01	White-light, Light Emitting Diode FRAMING Moving head fixture 
A.	General
1.	The fixture shall be a high-intensity white-light fixture with Cyan, Magenta, and Yellow subtractive color mixing and framing shutters. The fixture shall be a Lonestar by ETC or approved equivalent. 
2.	All LED moving light fixtures shall be provided by a single manufacturer to ensure compatibility.
3.	The fixture shall be UL 1573 listed for stage and studio use and comply with EN60598-2-17 standard per CE certification.
4.	The fixture shall comply with the USITT DMX-512A standard
B.	Physical or Mechanical
1.	The fixtures structural framing shall be constructed of rugged, 1/8” aluminum, free of burrs and pits and finished with a matte black powder coating.
2.	Outer covers of head and yoke shall be constructed of ABS plastic with fine textured black surface and fastened to the head frame with quarter turn fasteners.
3.	The fixture dimensions shall be 
a.	600 mm (23.6”) from base of the enclosure, to the tip of the lens baffling.  Fixtures that are longer than this dimension shall not be deemed acceptable. 
b.	367 mm (14.5”) across the exterior dimensions of the yoke
c.	The Electronics enclosure shall be 220 mm (8.7”) Wide 
d.	Head length 409 mm (16.1 ”) 
e.	Fixtures shall weigh 21.3 kg (47 lbs)
4.	The fixture shall be able to be either truss mounted or set upright on a stable surface. Fixture shall be suitably designed for operation over or under mounted on a truss perpendicular to the ground as well as outrigged parallel to the ground.
5.	The following shall be provided:
a.	The fixture must include nine (9) interchangeable rotating gobos with 17.5 mm outside diameter and 13 mm image area.  Fixtures that have less than nine rotating gobo patterns shall not be deemed acceptable.
1)	Rotating gobo systems must be able to index to any point on the 360 positioning of the gobo.  
2)	Rotating gobos must be interchangeable with glass and metal gobo patterns without permanent or semi-permanent modification to the wheels or cartridges.
b.	The fixture must include eleven (11) fixed gobos on a stamped gobo wheel. 
c.	CMY (Cyan Magenta Yellow) subtractive color mixing system 
d.	Ten (10) interchangeable colors including red, blue, green, yellow, orange, purple, TM-30 filter, lavender, half CTO, full CTO, and dark blue. Capable of split colors and linear indexed positioning.  Fixtures without color wheels shall not be deemed acceptable.
e.	Electronic Linear CTO from Native Color temperature minus 4800 K
f.	Fixture shall have 540 degrees of pan and 270 degrees of tilt.  Pan and tilt must be controlled with 16bit control and utilize encoder sensors to guarantee correct step position.
1)	Fixture shall have a pan speed of 2.30s for 360 degree movement
2)	Fixture shall have a tilt speed of 1.26s for 180 degree of movement.
3)	Pan and tilt locks that stop at 0, 45, and 90 degrees for service and handling. Pan and tilt locks are not intended to be engaged during transport in pre-rigged truss.
g.	Frost system with two different diffusion media that soften the edges of the projection on a surface and allows for variation in insertion speed. Fixtures that do not have two or more diffusion media shall not be deemed acceptable.
h.	Automated 3.8-55 zooming lens system. Fixtures that can not achieve a hard focus on the gate at less than 4 degrees shall not be deemed acceptable.
i.	Animation wheel that allows for continuous and uninterrupted motion in two directions and can be moved in/out of the beam.
j.	Two prisms including five facet prism and four facet linear. 
1)	Prism are index able, and continuously rotatable in both clockwise and counterclockwise directions. 
2)	Both prisms must be able to be inserted in the beam simultaneously. Fixtures that can not insert two prisms into the beam simultaneously shall not be deemed acceptable.

6.	The yoke arms must have collapsible, spring loaded, handles for fixture handling and manipulation.
7.	Power supply, cooling and electronics shall be integral to each unit.
8.	The unit shall ship with:
a.	5’ Neutrik True1 PowerCon™ to wire ferrule as standard
b.	Two (2) brackets that facilitate attaching standard brackets to the fixture base via ¼ turn thumb screws.
C.	Optical
1.	The light emitting diode engine shall produce 7000K white light within +/-500K out of the front lens of the luminaire
2.	The light engine shall be create color rendering at greater than 70 CRI 
3.	The fixture shall produce a maximum of 12,000 or greater field lumens while thermally stable and at full intensity.  Luminaires that reach 12,000 lumens only by integrating sphere or total lumen testing shall not be deemed acceptable.
4.	The unit shall provide, but not be limited to:
a.	Low gate and beam temperature
b.	Sharp Imaging on all gobo planes
c.	3.8 through 55 degree field angles
d.	High-quality pattern imaging throughout zoom range
5.	Fixture shall have two diffusions, one light and one medium, and have an option for a third diffusion, heavy, to be added without removing either of the other two diffusion options.
D.	Environmental and Agency Compliance 
1.	The fixture shall be ETL and cETL LISTED and/or CE rated, and shall be so labeled when delivered to the job site.
2.	The fixture shall be ETL LISTED to the UL1573 standard for stage and studio use 
3.	The fixture shall be rated for IP-20 dry location use.
4.	When the fixture is stationary, and at full intensity, the fixture may not produce noise in excess of 35 dBA.  A fixture that produces noise in excess of 35 dBA when stationary and at full intensity shall be deemed unacceptable. 
a.	At no time may the fixture produce noise in excess of 43 dBA.
1)	All dBA numbers above are tested in a test chamber with background noise level of 16.3 dBA.
5.	Fixture shall have linear fan control that allows a user to select fan speed level.  When this feature is active the luminaire may budget output as is necessary to maintain safe operating temperatures but may not change fan speed.  Fixtures that do not have linear fan control in this manner shall be deemed unacceptable.
E.	Thermal 
1.	Fixture shall be equipped with a heat pipe radiant cooling system.
2.	The fixture shall utilize advanced thermal management systems to maintain LED life to an average of 70% intensity after 20,000 hours of use 
a.	Fan speed will adjust automatically based on thermal management needs.
1)	Fixture will provide three fan speed modes that are selectable via DMX.
2)	Fixture will also provide a linear fan speed control channel.
b.	Thermal management shall include temperature sensors within the housing to include:
1)	LED array circuit board temperatures
c.	Fixture shall permit monitoring of temperature sensors via a legible LCD multi-line backlit display
d.	Fixtures that do not provide active thermal monitoring, fan speed controls, and current management of LED circuits shall not be acceptable.
3.	The fixture shall operate in an ambient temperature range of 0°C (32°F) minimum, to 45° C (113°F) maximum ambient temperature. During times of storage, the fixture shall be stored in temperatures range of -20C (0°F) to 60C (140°F)
4.	The fixture shall maintain .5 m (1.64 feet) distance from any flammable object
5.	The fixture shall maintain a minimum of 2.0 m (6.56 feet) to any lighted object.
F.	Electrical
1.	The fixture shall be equipped with a 100V to 240V 50/60Hz auto-sensing internal power supply 
a.	Fixture shall draw a maximum of 5.4 amps at 100V and 2.1 amps at 240 V.
2.	The fixture shall support power in and thru operation 
a.	Power in shall be via Neutrik® PowerCon™ True1 input connector
b.	Power thru shall be via Neutrik ® PowerCon ™ True1 output connector
3.	The fixture requires power from a non-dimmer source 
4.	Power supply outputs shall have self-resetting current-limiting protection
5.	Power supply shall have power factor correction greater than 0.97 from 100 VAC to 240 VAC.
G.	LED Emitters
1.	All LEDs used in the fixture shall be high brightness and proven quality from established and reputable LED manufacturers. 
a.	YLX is the sole manufacturer of approved emitter engines.
2.	Manufacturer of LED emitters shall utilize an advanced production LED binning process to maintain color consistency.
3.	All LED fixtures (100% of each lot) shall undergo a minimum 12-hour burn-in and stress test during manufacturing.
4.	LED system shall comply with all relevant patents
5.	Fixtures shall have PWM frequency up to 16,000hz to avoid flicker on camera
H.	Calibration
1.	Fixture shall be calibrated at factory to achieve consistent color and intensity output between fixtures built at different times and/or from different LED lots or bins
a.	All arrays, including replacement arrays shall be calibrated to the same standard to insure consistency.
I.	Color
1.	The fixture shall be available in specialized LED arrays as outlined below:
a.	Ultra-Bright 8000k white light engine
1)	White LED Engine calibrated and binned to achieve 8000k (+/- 400k).
a)	Measured brightness of Ultra-Bright 8000k engine installed in luminaire shall be greater than 15,400 Lumens when tested in an integrating sphere.
2.	Fixture must have a subtractive color mixing system utilizing six (6) dichroic color flags, controlled in pairs, to linearly subtract the following colors out of fixtures light output.
a.	Cyan
b.	Magenta
c.	Yellow
3.	Fixture must have semi trapezoidal dichroic glass color segments on a single wheel that transmit the following colors. Dichroics are permanent and mounted in place via adhesive.
a.	Red
b.	Green
c.	Blue
d.	Yellow
e.	Purple
f.	TM-30
g.	Lavender
h.	Half CTO
i.	Full CTO
j.	Dark Blue
4.	Fixture shall have an electronic CTO that utilizes the CMY mixing system of the fixture to reduce CCT color temperature from fixtures native color temperature down to 2200 K
J.	Dimming
1.	The LED system shall use 16-bit DMX control techniques for high-resolution dimming.
2.	Dimming curves shall be optimized for smooth dimming over longer timed fades. 
3.	The LED system shall be digitally driven using high-speed pulse width modulation (PWM)
4.	LED control shall be compatible with broadcast equipment in the following ways:
a.	PWM control of LED levels shall be imperceptible to video cameras and related equipment
K.	Control and User interface
1.	Ethernet compatible with support for ANSI1.31 Streaming ACN and ArtNet protocols
2.	Fixture must provide an internal ethernet switch that supports both active and passive data pass-through.
3.	Fixtures shall be support protocol conversion from Ethernet to DMX output and also conversion from DMX input to Ethernet output.
4.	The fixture shall be USITT DMX 512A-compatible via In and Thru 5-pin XLR connectors 
5.	The fixture shall be compatible with the ANSI RDM E1.20 standard
a.	All fixture functions shall be accessible via RDM protocol for modification from suitably equipped control console
b.	Temperature sensors within the luminaire shall be viewable in real time via RDM.
c.	Fixtures not offering RDM compatibility, feature set access or temperature monitoring via RDM shall not be compatible
6.	The fixture shall be equipped with multi-line color LCD display for easy-to-read status reports and configuration changes.
a.	Display must have a feature to battery power the menu structure when the fixture is unplugged to allow fixture settings to be adjusted, including DMX.
7.	The fixture shall be equipped with a six-button user-interface
8.	The fixture may offer two DMX control profiles.  
a.	Standard DMX Control Profile will have 39 channel control.
b.	Trifusion DMX Control Profile will have 39 channel control.