1.01	Remote Video Interface
A.	General
1.	The Net3 Remote Video Interface 3 (RVI3) shall be a microprocessor-based device specifically designed to provide display of system data for Eos Family lighting control systems.
2.	The RVI3 shall contain the operating software for all supported products and may be changed easily from one operating mode to another.
3.	Software updates shall be installed via USB flash drives.
4.	20 pre-programmed buttons shall be provided on the front panel of RVI.
5.	The unit shall support three external Display Port monitors, which may also be single or multi-touch displays.
6.	Four front panel LEDs provide operating status indication.
7.	A variety of different controls may be attached to the RVI3 via the USB ports on the back or front of the unit.
B.	Operation
1.	The RVI3 shall provide both remote viewing and remote programming of all show data. Only two external displays may be used when working with Gio @5, Ion Xe, Ion or Element.
2.	The RVI3 shall provide discrete local control, or may mirror other control device operations.
3.	The 20 buttons shall be remapped to provide access to any control keys.
4.	It shall be possible to connect the Net3 RFR, Eos Programming Wing and Motorized/Non-motorized wings.
5.	Monitor resolution shall be 1280x1024 minimum. The monitors may also be touchscreens or multi-touch displays.
C.	Interfaces
1.	AC Input
2.	USB (seven ports for items such as alphanumeric keyboard, pointing devices, touch screens, USB flash drive, etc.) 
3.	Ethernet (two discrete posts) 802.3af compliant PSE
4.	Three Display Port connectors at 1280x1024 resolution minimum, supporting standard, single or multi-touch displays
D.	Accessories
1.	Rack Mount Kit
2.	ETCpad (ETC Portable Access Device)
3.	20 Fader or 40 Fader non-motorized wings
4.	10 Fader or 20 Fader motorized wings
5.	Eos Programming Wing
6.	iRFR and iRFR Preview (application for Apple devices)
7.	aRFR (application for Android devices)
E.	Physical and Acoustical
1.	All controls and electronics shall be in a single enclosure, not to exceed 17.13” (435mm) wide, 15.88” (403mm) deep, 3.52” (89 mm) high, weighing 22.5 pounds (10.21 kgs). Device power shall be 90 – 240V AC at 50 or 60Hz, supplied via a detachable power cord.
2.	At typical CPU utilization, the unit shall operate at ≤ 30 dBA.