1.01	2.5 Watt Color mixing Light Emitting Diode fixture 
A.	General
1.	The fixture shall be a broad-spectrum color-mixing LED illuminator with DMX control of intensity as well as color changing. The fixture shall be a Vivid-R as manufactured by Electronics Theatre Controls, Inc. or approved equal. 
2.	All LED fixtures shall be provided by a single manufacturer to ensure compatibility. 
3.	The fixture shall comply with USITT DMX-512 A.
B.	Physical 
1.	The unit shall be black in color and contained in a rugged all-metal extruded and formed-metal housing, free of burrs and pits. 
2.	Power supply, cooling and electronics shall be integral to each unit.
3.	The unit shall provide, but not be limited to:
a.	1/2” Mounting bolts on each end
b.	5’ power lead with Edison connector
c.	Easy-access slots for secondary lenses for varied beam spreads
d.	Optional yoke (11” and 21” only), trunnion, and hanging bracket mounting kits. 
e.	Bare-end, Stage-Pin or Twist-Loc power leads shall be available
4.	Four sizes shall be available:
a.	11in (280mm) long by 7.1in (180mm) high by 7.1in (180mm) deep, with a weight of 11.5 lbs (5.2 kg) not including mounting hardware 
b.	21.5in (547mm) long by 7.1in (180mm) high by 7.1in (180mm) deep with a weight of 20 lbs (9.1 kg) not including mounting hardware
c.	42.5in (1080mm) long by 7.1in (180mm) high by 7.1in (180mm) deep with a weight of 35 lbs (15.9 kg) not including mounting hardware
d.	63.5in (1613mm) long by 7.1in (180mm) high by 7.1in (180mm) deep with a weight of 53 lbs (24.1 kg) not including mounting hardware
C.	Environmental and Agency Compliance
1.	The fixture shall operate in an ambient temperature range of 0°C minimum, to 40° C (104°F) maximum ambient temperature. The fixture shall be rated for IP-20 dry location use.
2.	The fixture shall utilize advanced thermal management systems for long LED life 
3.	The fixture shall provide on-board fan speed control
4.	LED fixture housing shall be designed to transfer heat from the LED board to the outside environment. 
5.	The fixture shall be ETL and cETL LISTED, and shall be so labeled when delivered to the job site. The fixture shall be ETL LISTED to UL1573. 
D.	ELECTRICAL 
1.	The fixture shall be equipped with 100V to 240V 50/60 Hz internal power supply 
2.	The fixture shall receive power via Neutrik® PowerCon™ input connector 
3.	The fixture requires power from non-dim source 
4.	Power/data supply outputs shall have current limiting protection.
5.	Power/data supply shall provide miswiring protection. 
6.	Power/data supply shall have power factor correction. 
7.	Power/data supply shall be UL listed for Class 1 or Class 2 wiring 
8.	Power/data supply shall come with a housing that meets a minimum IP20 rating for dry location installation 
E.	LED Emitters
1.	The fixture shall utilize red, red-orange, amber, green, cyan, blue, and indigo emitters for maximum spectral output.
2.	All LEDs used in the LED fixture shall be high brightness and proven quality from established and reputable LED manufacturers. 
3.	Manufacturer of LED systems shall utilize an advanced production LED binning process to maintain color consistency.
4.	LED emitters should be rated for nominal 50,000 hour LED life 
5.	The fixture shall utilize Luxeon® Rebel™ 2.5W LED emitters 
6.	All LED fixtures (100% of each lot) shall undergo a minimum eight-hour burn-in test during manufacturing.
7.	LED system shall comply with all relevant patents.
F.	Warranty
1.	The fixture shall be provided with the minimum warranty:
a.	5 years full fixture coverage
b.	10 years LED coverage
G.	COLOR 
1.	The fixture shall utilize the exclusive x7 Color System™ 7-color LED array 
a.	Each 11” cell shall contain 40 LEDs
b.	Each 11” cell shall contain seven different colors of LED emitters for maximum spectral output
2.	The fixture shall optimized for excellent pastel and saturated colors
3.	The LED system shall be capable of at least 15-bit control of each color level in each cell for greater than 1 billion possible color combinations.
4.	The fixture shall interact seamlessly with conventional sources 
5.	The fixture shall render light tints and skin tones similar to tungsten-sourced fixtures. 
H.	CONTROL 
1.	Each 11” cell of every fixture shall have the capability to be set to a unique and individual address. 
a.	21” fixture provides 2 independently controlled cells 
b.	42” fixture provides 4 independently controlled cells 
c.	63” fixture provides 6 independently controlled cells
2.	The fixture shall be DMX 512 compatible via In and Thru 5-pin XLR connectors 
3.	The LED system shall be digitally driven using high-speed pulse width modulation (PWM). 
4.	LED control shall be compatible to broadcast equipment
a.	PWM control of LED levels shall be imperceptible to video cameras and related equipment
5.	Each 11” cell of every fixture shall provide 8 channel control (7 color plus intensity) 
a.	An intensity channel shall be utilized for each cell to minimize color shift during dimming. 
6.	The LED system shall use 15-bit nonlinear scaling techniques for high-resolution dimming. 
7.	Dimming curves shall be optimized for smooth dimming at low intensities and over longer timed fades.